{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":51,"n_cols":6,"rows_kept":51,"merged":[[0,0,0,5]],"flags":["formulas_cached_only"]}
["淖尔壕煤矿采掘工作面支架、大巷延伸照明、地面照明改造灯具采购明细表"]
["序号","设备材料名称","型号","单位","数量","备注"]
["一","采掘工作面照明"]
[1,"矿用隔爆型LED支架灯","DGC48/127L(A)","盏",50,"灯体材质为铸钢件，详见技术要求"]
["二","东西大巷延伸"]
[1,"矿用隔爆型LED巷道灯","DGS48/127L","盏",70,"灯体材质为铸铝件，详见技术要求"]
["三","地面照明灯具",{"$nulls":3},"由中标单位负责安装，详见技术要求"]
[1,"单挑路灯太阳能支架","含电池板、蓄电池、控制器","套",21]
[2,"单挑路灯灯头","LED光源，DC12V，60W","套",21]
[3,"庭院灯（一体式）","含电池板、蓄电池、控制器","套",19]
["四","宿舍及办公楼等地点照明灯具",{"$nulls":3},"由中标单位负责拆除及安装，具体详见安装地点及要求统计表"]
[1,"LED平板灯","36W","盏",247,"高亮度白光"]
[2,"LED平板灯","24W","盏",328,"高亮度白光"]
[3,"LED吸顶灯","18W","盏",459,"高亮度白光"]
[4,"LED吸顶灯","12W","盏",134,"高亮度白光"]
[5," LED灯管","24W","根",70,"高亮度白光"]
[6," LED灯管","12W","根",226,"高亮度白光"]
[7,"LED泛光灯","100W","盏",30,"高亮度白光"]
[8,"LED泛光灯","200W","盏",5,"高亮度白光"]
[9,"LED泛光灯","400W","盏",10,"高亮度白光"]
["五","亮化字幕太阳能供电设备"]
[1,"1#宿舍楼亮化字幕",{"$nulls":3},"由中标单位负责安装，详见技术要求"]
[1.1,"光伏组件","单晶335W","个",70]
[1.2,"组件支架","平屋顶，倾角40度","组",70]
[1.2999999999999998,"光伏逆变器","额定功率25.5kW，MPPT范围150～1000V","套",1]
[1.3999999999999997,"充电控制器","最大输入功30kW，标称电压400V","套",1]
[1.4999999999999996,"蓄电池","12V，120Ah","块",32]
[1.5999999999999994,"直流配电箱","500*400*200*1.5mm,防护等级为IP65。含直流断路器、直流电压表","面",1]
[1.6999999999999993,"交流配电箱","500*400*200*1.5mm,防护等级为IP5。含交断路器、电能表","面",1]
[1.7999999999999992,"线缆及辅材","电缆、扁钢等","套",1]
[1.899999999999999,"支墩及储电池房","140个支墩，电池放1间","套",1]
[2,"2#宿舍楼亮化字幕",{"$nulls":3},"由中标单位负责安装，详见技术要求"]
[2.1,"光伏组件","单晶280W","个",30]
[2.2,"组件支架","平屋顶，倾角40度","组",30]
[2.3000000000000003,"光伏逆变器","额定功率10kW，MPPT范围180～500V","套",1]
[2.4000000000000004,"充电控制器","最大输入功率10kW，标称电压240V","套",1]
[2.5000000000000004,"蓄电池","12V，75Ah","块",18]
[2.6000000000000005,"直流配电箱","500*400*200*1.5mm,防护等级为IP65。含直流断路器、直流电压表","面",1]
[2.7000000000000006,"交流配电箱","500*400*200*1.5mm,防护等级为IP5。含交断路器、电能表","面",1]
[2.8000000000000007,"线缆及辅材","电缆、扁钢等","套",1]
[2.900000000000001,"支墩及储电池房","60个支墩，电池放1间","套",1]
[3,"办公楼亮化字幕",{"$nulls":3},"由中标单位负责安装，详见技术要求"]
[3.1,"光伏组件","单晶280W","个",24]
[3.2,"组件支架","平屋顶，倾角40度","组",24]
[3.3,"光伏逆变器","额定功率6.5kW，MPPT范围180～500V","套",1]
[3.4000000000000004,"充电控制器","最大输入功7.2kW，标称电压240V","套",1]
[3.5000000000000004,"蓄电池","12V，55Ah","块",18]
[3.6000000000000005,"直流配电箱","500*400*200*1.5mm,防护等级为IP65。含直流断路器、直流电压表","面",1]
[3.7000000000000006,"交流配电箱","500*400*200*1.5mm,防护等级为IP5。含交断路器、电能表","面",1]
[3.8000000000000007,"线缆及辅材","电缆、扁钢等","套",1]
[3.900000000000001,"支墩及储电池房","48个支墩，电池放1间","套",1]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}